To run the case run the Allrun script
To clean the case run the Allclean script

To post-process the data Matlab or python3 is required
    The matlabPost.m file post-processes the data and generates graphs of pressure and flow rate.
    The pythonPost.py file post-processes the data and generates graphs of pressure and flow rate.

To generate the transient valve sequence Matlab is required
    The exportValveData.m generates the transient valve sequence and print a figure.

Note that Matlab version R2021a Update 1 (9.10.0.1649659) was used for the Matlab scripts,
other versions may work but can not be guaranteed by the authors.

Note that Python version 3.8.10 [GCC 9.3.0] was used for the python script,
other versions may work but can not be guaranteed by the authors.

The validation data from Wang et al. (2017) and Petit et al. (2015) is found in validationData/
